//Logger //Sensor02

// sent Token to Sensor02 // received token

prepare message id: 4020101 Timestamp id : 2ff0101

OK Token received, start sending 10 msgs

//Sensor03

// no token, stops after timesync

Timestamp id : 2ff0101

//Logger //Sensor02

// receive 10 msgs from Sensor02 // send 10 packages to logger

Sensor data: 055f7cf52602e Impact complete:

Sensor id : 1c010201 Starttime: 5633999

Sensor len : 8 Samples: 46

. Peaks: 6

. Maximum: 594

. \*\*\*\*\*\*\*\*\*\*\*

. sent payload 055f7cf52602e

. OK, Message sent to logger

.

. Impact complete:

. Starttime: 5829023

. Samples: 36

. Peaks: 5

. Maximum: 260

. \*\*\*\*\*\*\*\*\*\*\*

. sent payload 058f19f45024

Sensor data: 058f19f45024 OK, Message sent to logger

Sensor id : 1c010201 Token revoked

Sensor len : 8

//Logger //Sensor03

give token to SensorID 3 of 2 Timestamp id : 2ff0101

prepare message id: 4030101 Token received, start sending 10 msgs

OK

Impact complete:

Starttime: 11874290

Samples: 1

Peaks: 1

Maximum: 410

\*\*\*\*\*\*\*\*\*\*\*

sent payload 0b52ff29a101

Sensor data: 0b52ff29a101 OK, Message sent to logger

Sensor id : 1c010301 Token revoked

Sensor len : 8

Impact complete:

give token to SensorID 2 of 2 Starttime: 12065974

prepare message id: 4020101 Samples: 25

Peaks: 6

Maximum: 334

\*\*\*\*\*\*\*\*\*\*\*

sent payload 0b81cb64e6019

No token, message stored